**Flat-Felled Seam**

A flat-felled seam is self-enclosed (therefore a seam and seam finish within itself) and requires no additional seam finishing technique. Use it where durability is needed or a tailored appearance is desired.

1-With the wrong (back) sides of the fabric together, make a plain seam. Press seam allowances in one direction.

2-Trim the under seam allowance to 1/4 inch. It is really important to get this correct!

3-On the remaining seam allowance, turn under 1/4 inch and press. Fold this side over the trimmed edge. Pin in place.

4-Stitch very close to the folded edge of the seam allowance.

5-Staple your example to this paper and turn in at the front of the room.