**Machine Hem Sample**

(Follow the directions on your guidesheet. They may differ from this method.)

Use directions 1-5 on the front of this page (Casing Sample). Do not cut the elastic for this sample. This time, continue sewing until your stitching overlaps. Do not leave the 1” gap.