**Pinked Seam Finish**

Pinked seam finishes look nice, but they are not to be used on fabrics that ravel easily.

Follow these steps to make a Pinked Seam Finish sample:

**You will need 2-4” by 8” pieces of sample fabric for this seam.**

1-With the right (front) sides of the fabric together (along the 8” sides), make a plain seam.

2-Press your seam open pulling it flat all the way to the stitches on both sides. (You should not have a crease near the seam.)

3-Pink the edges of the seam allowances (with the pinking shears provided) separately lining up the zigzags each time you cut as to make them look as consistent as possible. Try to cut as little as possible off of your seam allowances.

4-Press your seam flat again.

**\*\*\*Staple your finished sample to this page and turn it in to the bin for your class period at the front of the room.\*\*\***