**Stitched and Pinked Seam Finish**

The stitched and pinked seam finish will improve the durability and help prevent raveling of the regular pinked seam.

Follow these steps to make a Stitched and Pinked Seam Finish sample:

**You will need 2-4” by 8” pieces of sample fabric for this seam.**

1. Stitch a regular 5/8” seam.
2. Press the seam open.
3. Stitch 1/4" from the edge of each side of the seam allowances. (Do not sew through to the outside of the fabric.)
4. Pink the seam allowance.
5. Press the seam open once more.

**\*\*\*Staple your finished sample to this page and turn it in to the bin for your class period at the front of the room.\*\*\***