**Turned and Stitched Seam Finish**

This seam finish looks neat and prevents raveling. It is often used for unlined jackets of lightweight fabrics. It is also used on the edges of facings for sheer and lightweight fabrics. It is too bulky for medium and heavy weight fabrics.

**You will need 2-4” by 8” pieces of sample fabric for this seam finish.**

1. Sew a regular 5/8” seam.
2. Press the seam open.
3. Turn the edges of each seam allowance under ¼”. Press.
4. Stitch close to the fold on each seam allowance. **DO NOT** SEW THROUGH SO THAT IT SHOWS THE OUTSIDE OF THE SEAM. You are just sewing the seam allowances on this step.

**\*\*\*Staple your finished sample to this page and turn it in to the bin for your class period at the front of the room.\*\*\***