**Machine Hem Sample with 5 “Nametags”**

1-Cut a rectangle of fabric 15” x 5”.

2-With right sides together, pin and then sew the two 5” sides together.

3-Be sure to finish the seam edges in some way (serge, zig zag the edges, use pinking shears, etc.)

4-Using a seam roll or sleeve board, turn the top edge of your loop down 1 1/2” and press. Turn under the raw edge ¼” and press.

5- Pin this folded edge down around your sample. Starting at your previous seam, stitch close to the edge around your loop. Be sure to backstitch.

6-See me for a demo of sewing in nametags if you need to. I would like for you to sew in 5 in the inside of the hem for practice (we can pretend it is a waistband). You may use pinking shears on the ends so they do not continue to un-ravel or you can tuck the top under and press if you would like.

7-Staple this sample to this paper and turn it in to the bin at the front of the room.